千通AC功能
[bookmark: _GoBack]一、AP和AC之间的接口协议
AP和AC之间通过MQTT协议对接，AP是client端，AC是server端，TCP端口是5247。MQTT之上是ProtoBuf协议，ProtoBuf具体定义在《mqtt对接文档》中；
二、工作流程
1. AP和AC之间链接建好之后AP订阅如下几个topic：
AC/%s/M_WRconfig    // 中间填充AP序列号
AC/%s/M_cmd        // 中间填充AP序列号
AC/%s/M_lists        // 中间填充AP序列号
2. AP定期发布AP/echo这个topic，携带AP自己的信息以及终端的信息；
三、AC实现的功能
1. 千通AC目前实现了部分AP管理功能和DHCP功能；
2. DHCP支持动态IP配置和静态IP配置，通过配置文件配置；
3. 管理功能目前通过telnet来完成，方法如下：
# telnet localhost 4100
[image: 1731578612157]
1） 显示所有AP列表
AC> list ap
[image: 1731578715898]
2） 显示所有终端列表
AC> list subs
[image: 1731578767938]
3） 重启AP
AC> reboot #apSn
[image: 1731578984225]
4） 下线某个终端
AC> kick #apSn #staMac
[image: 1731578952803]
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agtuser@eNR174:~$ telnet localhost 4100

Trying 127.0.0.1...
Connected to localhost.

Escape character is '~]".

AVAILABLE COMMANDS

kick #apSn #staMac

Kick the STA specified by mac.

| Command | Remark |
help | Help page.
date | Current date.
list ver | Display version information.
list ap | List all APs.
| List all wifi subscriber data.
|
|

reboot #apSn

|

|

|

|

| list subs
|

|

| set #ssid #passwd
|

debug level error/warn/info/debug/trace | Set debug level.

| q or quit

Reboot the AP specified by SN.

Set wifi ssid and password.

Quit.

acs [
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AC> list ap

s BELH FIS TiEER mAmR IPHE MACH: 5 BES
BL60OOX AP BL6000X0247120159 FIT AP dhcp 172.16.11.116  04:C3:E6:69:06:48 6Day 6hllm
Ac> []
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AC> list subs B
TP AL MACH: 3 EHE

HE  FBAP FURAPETS AP HAC THLH ESBEE BUEE RHES
172.16.11.21  d2:ab:13:8a:e8:15 ANA-ANOO 2.4G BL600OX0247120159 AP 6:69:D6:48 yh-test -37 dBm  103.1 114.1
172.16.11.20  42:9c:aa:1b:87:d5 NOP-ANGO-PD 2.4G BL600OX0247120159 AP 6:69:D6:48 yh-test -44 dBm  143.1 129.1
Ac> []
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AC> reboot BL6000X0247120159
COMMAND 0K
Ac> []
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AC> kick BL6000X0247120159 d2:ab:13:8a:e8:15
COMMAND 0K
Ac> []




